Wichtige Befehle der LCD Bibliothek

/**
* Set the LCD display in the correct begin state, must be called before anything else is done.
*/
void begin();
/**
* Remove all the characters currently shown. Next print/write operation will start
* from the first position on LCD display.
*/
void clear();
/**
* Next print/write operation will will start from the first position on the LCD display.
*/
void home();
/**
* Do not show any characters on the LCD display. Backlight state will remain unchanged.
* Also all characters written on the display will return, when the display in enabled again.
*/
void noDisplay();
/**
* Show the characters on the LCD display, this is the normal behaviour. This method should
* only be used after noDisplay() has been used.
*/
void display();
/**
* Do not blink the cursor indicator.
*/
void noBlink();
/**
* Start blinking the cursor indicator.
*/
void blink();
/**
* Do not show a cursor indicator.
*/
void noCursor();
/**
* Show a cursor indicator, cursor can blink on not blink. Use the
* methods blink() and noBlink() for changing cursor blink.
*/
void cursor();
void scrollDisplayLeft();
void scrollDisplayRight();
void printLeft();
void printRight();
void leftToRight();
void rightToLeft();
void shiftIncrement();
void shiftDecrement();
void noBacklight();
void backlight();
bool getBacklight();
void autoscroll();
void noAutoscroll();